**Slot It Models Allowed**

* Alfa Romeo 155 V6Ti
* Mercedes 190E
* Opel Calibra

**Body**

* Modifications prohibited (except as follows)
* OEM hard cockpits and Glass mandatory; Lexan cockpits prohibited.
* Body must start every race with all major parts intact (e.g. windows and wings).  Antennas, mirrors, wipers, tow hooks, and other small parts damaged from accidents do not have to be replaced.
* Wings mandatory at the start of a heat.
* White kits allowed – but must be painted (or decaled uniquely) with at least one coat of paint.  At least two numbers must be visible.
* Body screws open choice.
* Body screws may be taped to prevent loss. If a screw falls off the car and causes an issue with a competitor’s car, Five lap penalty applied.

**Chassis**

* No modifications to chassis allowed unless otherwise specified.
* Only the stock OEM Slot.It chassis for the model is allowed.
* Chassis must be of type intended for body.
* Only flashing on chassis may be removed to allow better floating of the body. Gaps between the chassis and body that are larger than the width of a credit card - .085mm - will not be allowed.
* Cars must have sufficient ground clearance to permit free running without contacting track. Cars should have a minimum of 0.50mm ground clearance.
* Front axle lower adjustment caps allowed. Modification to the upper axle loops is prohibited.
* Slot It bushings are allowed for the front axle.
* Slot.It guides mandatory – SICH-07 deep wood screw guide highly recommended.
* Pick-up braids open choice.
* Traction magnets prohibited.
* Ballast allowed; mustbe above the chassis pan. 5 lap penalty will be imposed if ballast falls onto track and causes an issue with a competitor’s car.
* Lead wires – free choice.
* Wheel/tire must not we visible outside wheel-well/fender when viewed from above.

**Motor**

* The stock Slot.It 21Kblack end-bell motor mandatory.
* Modifications to motor are prohibited with the exception of removal of the circuit board on top of the motor.

**Motor Pod**

* Only the stock CH-110 OEM motor pod is allowed.
* Motor pod prohibited from protruding below chassis.
* Only flashing may be removed from motor pod to allow better float. Excessive removal of material determined by scrutineer.
* Spacers/washers open choice.
* Slot.it spherical bushings mandatory.
* Pod screws are open choice.
* Tape may be used to prevent the Pod Screws from falling out.

**Gears**

* Slot.Itin-line gears and pinions mandatory.
* Gear Ratio open-choice.
* Modifications to Crowns or Pinions prohibited

**Wheels**

* Only the stock Slot.it short hub aluminum 15.8 x 8.2 wheels allowed on the rear.  Front wheels must be stock 15.8 x 8.2 plastic or the aluminum versions of the same dimension.
* Slot.it wheel inserts are mandatory.
* Inserts may be interchanged from different models.
* Modifications prohibited.

**Axles**

* Only Slot.It axles allowed.  Modifications to axles prohibited.
* Independent front axles are prohibited.

**Tires**

* Only Slot.It tires are allowed.
* Tires may be glued to the wheels, trued and have their edges rounded.
* Tires cannot be trued in a conical shape where one edge is larger than the other.
* Traction compounds prohibited.
* Nail polish on front tires is prohibited.

**Track Power:    12v**

**General**

If it is not mentioned it is not legal.  These rules were written to create a fair event and not for racers to look for loopholes.